
Composite Interlocking Deck Tiles Installation Guide


1. Calculate the area of your project and double check the order amount:
   1. Length x Width = Area (in2)
   2. Area(in2) /136.59375 (in2) = Number of Tiles

Note: Individual tiles are 12.2”x12.2” squares but the Exposed surface of each tile is ~ 11.875” x 11.875”


Groove

Tongue



**Installation:** Click Tiles together in the patern of your choice. ( Note: to keep lines straight, Start in a corner or in the center of the longest wall and work outwards)

**Trimming Tiles to size:** Mark the size along the bottom mat, (avoiding the screws) cut the tile to size using a hand saw.

Opposing Pattern Long Pattern

1. The distance of at least 1 inch from walls or other obstacles for a 16” long installation to allow for expansion of the interlocking composite DIY tiles is necessary at installation